Mini Wishing Well

STEP 1

Fasten the four 1 X 8 - 12" together

to form base with 1 3/4" screws

STEP 2

Fasten the two 1 X 3 - 30" to base,

centered on opposite sides with

1 1/4" screws from inside.

Fasten the 14" lath pieces to top of base.

STEP 3

Attach 1 X 2 - 12 3/4" and 12" rafters to top of 1 X 3 , keeping them flush with outside with 1 3/4" screws.

STEP 4

Fasten 1 X 2 - 7" braces with 1 1/4" screws as shown in

fig. 1.

STEP 5

Attach 1 x 2 - 16" roof boards to rafters with 1 1/4"

screws as shown in fig. 1.

STEP 6

Select enough shingles to cover one layer of each side

of roof allowing shingles to over-hang roof boards by

aprox. 1". Cut 5" off the butt end and save for later.

Use the remainder of the cut shingles for first row,

overlapping gables and eaves by 1". Lay another

layer of shingles over first. Lay a second layer spaced

5" from the first , the thin ends will have to be trimmed on

these. Apply the third layer using the 5" butts cut from the

first layer.

STEP 7

Apply the 15" lath to trim gables, and 18" lath to trim peak.