BIRD FEEDER

> > This is a great project that your fine feathered friends will appreciate that you made. A fairly simple project, but very gratifying.

> > MATERIALS LIST

> > A.- Front 1/2" x 6 1/2" x 18" redwood (1)

> > B.- Back 1/2" x 5 1/2" x 18" redwood (1)

> > C.- Side 1/2" x 6" x 15 1/4" redwood (2)

> > D.- Bottom/Divider 1/2" x 5 1/2" x 5 1/2" redwood (3)

> > E.- Roof 1/2" x 6 3/8" x 8 1/2" redwood (1)

> > F.- Roof 1/2" x 5 7/8" x 8 1/2" redwood (1)

> > G.- Perch Rod 1/4" dia. X 2 1/2" birch (3)

> > E.- #8 x 1 1/4" Flathead Screws (80 - 100)

> > F.- Eye Hook (1) about a 1/4" x 2"

> > Click on the picture to get the full picture.

> > CONSTRUCTION

> > Begin construction by cutting out all the parts as specified in the materials list.

> > NOTICE:

> > There is no need to miter the roof (E, F), But the sides are mitered to 45 degrees.

> > Use a compass to draw the three 4" diameter holes on the front (A). Then drill starter holes and cut out the waste area using a jig saw or scroll saw.

> > Next drill the 1/4" diameter by 1/2" deep holes in which you will insert the perch rod (G).

> > Locate these holes to suit.

> > Now assemble the project using #8 x 1 1/4" brass flathead screws ( countersunk). Begin by attaching the bottom/divider (D) to the sides (C) and back (B) with wood screws. Then attach the front (A) and the roof (E, F).

> > Finally insert the perch rods (G) to complete the basic unit.

> > FINISHING

> > Thoroughly sand all of the parts, smoothing all of the sharp edges.

> > A finish is not necessary due to redwood is naturally weather resistant. However, if desired, you can apply a clear oil stain or several coats of an exterior grade varnish.

> > Complete the project by installing an eye hook in the top of the roof and inserting your choice of bird feed in the holes.

> > Now all that's left is to hang the feeder where desired and watch you fine feathered friends as they have a treat.