Plant Pokes

Materials Needed | Equipment Needed

¾" thick plywood Various colors of acrylic paint | Saber saw or similar product

Directions

Print template and enlarge if necessary

1. Cut pattern from ¼" thick plywood or wood of choice.
2. Print, trace and cut out characters.
3. Paint as desired or use colors chosen on template.
4. Drill a hole in the bottom edge of each yard character.
5. Insert 1/8" in diameter steel rod, dowel, pvc pipe or product of your choice approximately 8" in length.
6. Push rod into potted plant or yard.

Pattern Below