# Wine Rack

Material List

12 – 1 ¾” x 12” hardwood squares

5 - ¾” x 36” dowels

1) End trim 1 ¾” squares to 10 ½” in length.

2) Put a 3/8” radius on all sides and both ends of squares as per illustration F.

3) Drill 3’4” holes 1 ¼” inches from both ends and 9/16” deep (critical) as per illustration A, B & C.

A | B | C
2 required | 7 required | 3 required

4) Cut six legs from the ¾” dowels 2” in length as per illustration E.

D | E

5) Cut 32 pieces 4 ½” long from the ¾” dowels. See illustration D.

6) Sand and assemble.

Tips

1) It is best to assemble prior to staining.

2) Assemble all horizontal dowels first.

3) Gluing may/may not be necessary.

Front View | Exploded View
Top View | Exploded Top

##