Saucepan Hanger

Our frame measures 100mm x 450mm deep, but vary this to suit your needs. This simple frame is great for fixing into a spare corner close to the stove, or you can hang it from the ceiling
You'll need
100mm x 50mm dressed oregon, lengths to suit
Epoxy resin for gluing
8 x 100mm dowels
Hooks
Rope
Here's how
1. Measure out the size of your frame and cut to size.
2. Mitre and join the corners with epoxy resin and two dowels, sanded flush with the surface.
3. Screw in hooks.
4. Fix to the wall using appropriate fasteners, or suspend on chains from a large hooks screwed into the ceiling and the beams.
Tip
Keep lids under control with a length of rope knotted around dowels partially driven into the wall.